1000 Gallon LDHPE Vertical Storage Tank w/ 16" Manway SG-1.5, Size  64" dia. x 7’9” ht., 
 2" Polyurethane Foam Insulation with Two Latex Mastic Protective Coatings, 2" PVC sch 80 Bolted fitting.
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