**DILO RECLAIM TRAILER**

**Description of Items**

|  |  |  |
| --- | --- | --- |
| Mobile circuit breaker gas (SF6/CF4) Filling Unit | 1 |  |
| Custom rack to hold glass plant and, mixing tank | 3 |  |
| N150 cylinder with weight scale | 1 |  |
| Wall mounted, single cylinder scale for "waste gas" | 1 |  |
| Wall mounted holder for 2 cylinders for New SF6 & New CF 4 bottles | 1 |  |
| -1024-R050 - 5m/15' long wire braided hose DN 20 with Dilo DN 20 | 4 |  |
| ML1-AD22-55 2.0401 - Double stud DS 20 3 | 3 |  |
| T-81875-140 | 1 |  |
| TDP - trailer deluxe package | 1 |  |
| 240VAC Forced air heater - 5600 watt, 23.4A (MMC-3688K72) | 2 |  |
| MEC35DO - 35kW diesel generator set. Includes customized controls, fuel cap, battery, 20 foot cable | 1 |  |